

**NVR8916K-Q**

H.265 8 SATA Poe NVR K Series

**Parameters：**

**Features：**

|  |  |  |
| --- | --- | --- |
|  | **Model** | **NVR8916K-Q** |
| System | processor | Hi3536 |
| system | Embedded Linux |
| Video | Video input | 8ch4K/16ch5M/16ch3M |
| Playback | 2ch4K/4ch5M/8ch3M |
| Decode | H.265+/H.265/H.264 |
| Audio | Compression | G.711a |
| Intercom | Support |
| Management | Record mode | Manual>Alarm>Motiondetection>Timing |
| Inquire mode | Inquire by Time/Calendar/Event/Channel |
| Storage mode | HDD Storage, Network Storage |
| Backup | Network, USB, SATA |
| Interface | HDMI output | 1\*HDMI (MAX:4K) |
| VGA output | 1\*VGA (MAX:1080P) |
| Ethernet port | 1\*RJ45 1\*10/100/1000Mbps Ethernet port, |
| POE ports | 16 standard POE ports |
| Audio I/O | 1/1 |
| Alarm I/O | 0/0 |
| USB Port | 1\*USB2.0 ports，2\*USB3.0 ports |
| HDD | 8\*SATA interface (Up to 8TB) |
| General | Temperature | 0 ℃ - + 55 ℃ |
| Humidity | 10% -90% RH |
| Power supply | ATX(100-240V) |
| Consumption | <10W（Without HDD） |
| Weight | Around 6.0KG |
| Dimension | 443(L)\* 427.5mm(W)\* 92mm(H) |

* 8ch4K/16ch5M/16ch3M video input;
* HDMI/VGA simultaneous video output;
* 2U Case, 8SATA(Up to 8TB);
* H.265+/H.265/H.264
* 1\*10/100/1000Mbps auto-sensing Ethernet port, RJ45 port；
* Automatic networking support, a key to add equipment;
* Support the Onvif protocol;
* Support GB28181 (Optional);
* Cloud services, P2P, alarm information push to phone;
* Support remote access, support ARSP;
* "Support DHCP, FTP, DNS, DDNS, NTP, UPNP, EMAIL,
* 3G, WIFI, IP search, Alarm center, etc ;"
* Mobile phone remote monitoring (iOS, Android);
* Multi browser access (IE, Chrome, Firefox, Safari);
* Support for more than twenty languages;
* Perfect protection circuit, unique triple watchdog function;
* Support WEB, CMS, VMS, MYEYE Platform;

**Model：**

**NVR8916K-Q**

**Interface：**

****